HVAC and DWH Ratings Estimates
Heat Pump Ratings
	Year
	Pre 1992
	1992-2006
	2007-2015
	2016-2023
	After 2023

	HSPF
	5
	6.8
	7.7
	8.2
	N/A

	HSPF 2
	N/A
	N/A
	N/A
	N/A
	7.5

	SEER
	6
	10
	13
	14
	N/A

	SEER 2
	N/A
	N/A
	N/A
	N/A
	14.3



Packaged Units Manufactured after 2023 have a SEER 2 rating of 13.8

Condensing Unit Ratings (Central Air)
	Year
	Pre 1992
	1992-2006
	2007-2015
	2016-2023
	After 2023

	SEER
	9
	10
	13
	14
	N/A

	SEER 2
	N/A
	N/A
	N/A
	N/A
	14.3



Condensing Units with an output of 45,000 BTU (4 tons) have a SEER 2 rating of 13.8

Electric Furnace Ratings
	KW
	5
	10
	15
	20
	25
	30

	BTU
	17,000
	34,000
	51,000
	68,000
	85,000
	102,000



All Electric Furnaces will have an efficiency rating of 98%

Gas Furnace Ratings
	AFUE
	70%
	80%
	90%

	Description
	Natural Draft Furnace (No Motor on Flue)
	Inducer Motor with Metal Pipe Venting the Flue Gases
	Inducer Motor and PVC Pipe Venting the Flue Gases



You can also use the SSE (%) readings from your combustion analyzer.


Electric Water Heater Ratings
	Brand
	Energy Factor
	First Hour
	Input KW
	Recovery

	Rheem
	0.93
	62
	4.5
	98

	AO Smith
	0.93
	60
	4.5
	98

	Whirlpool
	0.93
	58
	4.5
	98

	US Craftmaster
	0.93
	58
	5.5
	98



Other manufacturers should have similar ratings. 

Gas Water Heater Ratings
	Year
	Energy Factor
	First Hour
	Input BTUs
	Recovery

	Pre 2020
	0.70
	67
	40,000
	75

	2020 or Later
	0.90
	86
	40,000
	92






*Note the ratings for HVACs and DWHs on this form are estimates for situations where the true ratings cannot be obtained due to age and/or deterioration of the system. If the model number and brand can be obtained, use other resources (Google) to determine these inputs. Always document the state of the current system with photos to justify your decision.*
